

when ping from one LAN to another it shows rQ timed out



if the ip address helper is not added you get DHCP failed





Router#configure terminal

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#int fa4/0 ->>> this is the router ip address

Router(config-if)#ip helper-address 10.0.0.2 ->>> this is the server ip address

Router(config-if)#exit

Router(config)#

Do the same for the all sides of the topology

1. Create topology

2. Select DHCP option in all the end devices for ip terminal

3. Satic routing for router, and for server

4.In server in services "on" DHCP

5.In services of server give default gateway as the router interface ip address of that side